#### BOAT/ASSETS

Home

#### 16M Crew/ Cargo boat

#### 12M SEABUS

#### 15M Pilot Boat

#### 12M Passenger boat

#### SP Nabalu 1

#### Yokohama Fender

## 16M Crew/ Cargo boat

### SRI PERKASA 81

###

#### Technical Data

- Construction material - Marine grade aluminium
- Construction standard - Structures designed and built to BV standard

- Dimensions (L x B x D) - 16.00 x 4.50 x 1.65 metres
- Engine - Daewoo L086TIH x 2 units rated 285BHP @ 2,100 rpm
- Draft - Hull- 0.9 metres
  Propellers- 1.4 metres
- Tonnage - Gross- 23.8 tonnes Net- 7.14 tonnes
- Displacement - Lightship- 13.5 tonnes Loaded- 16.4 tonnes

- Cargo Deck Area - 28sqm
- Exterior features - Remote Searchlight, DD Fenders, Fairleads, Bollard, Sand Anchor, Safety handrails

- Length Waterline - 15.2metres
- Gearbox - ZF IRM 280-1A (Ratio 2.476: 1) x 2 units
- Propulsion - Marine diesel driving propellers
- Speed - Max- 22 knots at full load w/o cargo

- Interior features - Plasticseats, Air-conditioned, Toilet, Escape hatch
- Safety - Lifebuoys, Life jackets, Fire extinguishers, First aid kit, Bilge Alarms,Others complied to marine department

Close

x

## 12M SEABUS

### SP MERCURY

###

#### Technical Data

- Construction material - Marine grade aluminium
- Construction standard - Vessel structure is to be designed to DNV High-Speed Craft Rules

- Length Overall - 13.00 metres
- Engine - DaewooL086TIHx 2 units rated 210kW@ 2,100 rpm
- Hull Length - 12.00metres
- Gearbox - ZF 286 (Ratio 1: 1) x 2 units
- Propulsion - Doen DJ120Z waterjet x 2 units

- Beam - Moulded - 3.30 metres
  Chine – 3.10 metres
- Draft - 0.60 metres
- Speed- Max- 28 knots full load, Cruise - 20 knots
- Navigation Aids - GPS + chart plotter, Marine radar, Depth sounder, Marine VHF fixed station, LED Navigation lights

- Range - 240nm at 20 knots
- Displacement - Light - 7.5 tonnes, Loaded- 9.3 tonnes
- Capacity - Crew- 2 pax, Passengers- 12 pax, Fuel-840 litres, Water- 100 litres

- Interior features - Fully LED lightings, Cushionseats, V berth cushion, Air-conditioned
- Exterior features - Remote Searchlight, Toilet, Floodlights, Wipers, Forward boarding door, Bollards, Safety handrails
- Safety - Lifebuoys, Life jackets, Fire extinguishers, First aid kit, Fuel cut off system & fire dampers,Others complied to marine department

Close

x

## 15M Pilot Boat

### SP87 Pilot Boat

###

#### Technical Data

- Construction material - Solid GRP hull, sandwich GRP deck and cabin
- Construction standard - Structure to Australian standard AS. 4132

- Dimensions (L x B x D) - 15.77 x 3.73 x 2.13 metres
- Engine - Doosan MD196TI 320ps @ 2,000rpm x 2 units
- Draft - 1.00 metres
- Gearbox - ZF305-2A, ratio1.514: 1 x 2 units
- Displacement - 11 tonnes

- Navigation Aids - Garmin GPS + chart plotter, Garmin Marine radar, Garmin Depth sounder, IcomMarine VHF fixed station, DHR Navigation lights,
- Exterior features - JabscoRemote Searchlight, Rubber DD Fenders, Bronze Fairleads, S/S Bollard, S/S Sand Anchor, Safety handrails

- Capacity - Passengers- 12 pax, Fuel-1,200 litres, Water- 100 litres
- GRT/NT - 26.58/ 7.97 tonnes
- Propulsion - Marine diesel driving propellers
- Speed - Max- 25 knots , Cruising- 20 knots

- Interior features - PVC covered cushions, Air-conditioned, Safety handrails, Lavatory, Escape hatch
- Safety - Lifebuoys, Life jackets, Fire extinguishers, First aid kit, Bilge Pumps with automatic switch
- Builder - Vigormax (M) Sdn. Bhd.

Close

x

## 12M Passenger Boat

###

#### Technical Data

- Construction material - Solid GRP hull, sandwich GRP deck and cabin
- Construction standard - Structure to Australian standard AS. 4132

- Dimensions (L x B x D) - 12.40 x 3.56 x 2.13 metres
- Engine - Volvo Penta D7-CTA x 2 units rated 265BHP @ 2,300 rpm
- Draft - 1.00 metres
- Gearbox - ZF IRM 280 A (Ratio 1.769: 1) x 2 units
- Displacement - 10 tonnes

- Navigation Aids - GPS + chart plotter, Marine radar, Depth sounder, Marine VHF fixed station, Automatic identification system(AIS) transponder, Navigation lights
- Exterior features - Remote Searchlight, DD Fenders, Fairleads, Bollard, Sand Anchor, Safety handrails

- Capacity - Passengers- 12 pax, Fuel-1,200 litres, Water- 100 litres
- GRT - 26.58 tonnes
- Propulsion - Marine diesel driving propellers
- Speed - Max- 25 knots , Cruising- 20 knots

- Interior features - PVC covered cushions, Air-conditioned, Safety handrails, Toilet, Escape hatch
- Safety - Lifebuoys, Life jackets, Fire extinguishers, First aid kit, Bilge Alarms Others complied to marine department
- Builder - Vigormax (M) Sdn. Bhd.

Close

x

## SP Nabalu 1

x